Wizard 8k9k Version 1.0.0.0 Release Candidate
=============================================

Build 920

December 18, 2008

- When the VIP/Fax line is not setup, one cannot make outbound calls from FXS1 and FXS2. Fixed.
- Automatically uncheck "Enable NAT Keep Alive" when "Enable NAT Mapping" is unchecked.
- Default ring time and maximum ring time changed to 8 and 20 seconds respectively.
- Added option to exclude the "No Answer Extension" from the hunt group.
- Enabled MOH for FXS1 and FXS2.
- FW upgrade check is now part of the discovery process.



Wizard 8k9k Version 0.9.1.0
===========================

Build 880

Sep 23, 2008

- Using latest FW for SPA9000 (6.1.5) and SPA8000 (6.1.3).
- Changed all Linksys to Cisco, including the working directory and registry key.
- Added Auto Attendant option.
- Added Unicode support.
- Added "Preview" buttons. No more forced previews of changes.
- MOH is now enabled.
- Now using static IP for the SPA8000's. This is needed for AA prompt download. This also speed things up significantly when saving system configuration changes.
- When VIP/Fax line is not setup and AA is not used, ext 201/202 is added to the hunt group.
- Many bug fixes.



Wizard 8k9k Version 0.9.0.2
===========================

Build 788

July 25, 2008

- The explicit routes set up to reach beyond the first SPA8000 are now persistent routes.
- On some PCs with virtual network adapters, the Wizard might crash during the device discovery process. Fixed.




Wizard 8k9k Version 0.9.0.1
===========================

Build 734

July 9, 2008

- When the PC on which the Wizard runs has multiple network interfaces, depending on the PC routing table the Wizard may not be able to reach beyond the first SPA8000 that is directly connected to the PC. This is solved by having the Wizard set up explicit routes for the second SPA8000 and devices beyond.

- The latest SPA8000 firmware, version 6.1.2, is included.




Wizard 8k9k Version 0.9.0.0
===========================

Build 648

June 12, 2008

- Can support up to three SPA-8000s (while only advertising two in the instructions).
- See "Wizard 8k9k Functional Specification.doc".
- Please send bug reports and comments to mingch@cisco.com.
